|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Списък на резервни части и консумативи** | | | | |
| № | Описание на оборудването | Ед. Мярка | Количество | Единична цена (в лв. без ДДС) |
| **1.0** | **HP ProLiant DL380p Gen8** |  |  |  |
| 1.0.1 | Power Supply HP Server 750 Watts |  |  |  |
| 1.0.2 | Processor HP Server; processor speed 2100 MHz, 6/6 cores, 12 threads; 64-bit Capable memory technology; internal cache - L1 192KB, L2 1536KB, L3 15360 KB. |  |  |  |
| 1.0.3 | Memory HP Server - size 8192 MB; frequency 1600 MHz |  |  |  |
| 1.0.4 | iLO 4 Dedicated Network Port |  |  |  |
| 1.0.5 | NIC HP Ethernet 1Gb 4-port 331FLR Adapter |  |  |  |
| 1.0.6 | HP Smart Array P420i Controller; Cache Module Memory - 1048576 KB |  |  |  |
| 1.0.7 | Physical Drives, Capacity 279 GB |  |  |  |
| **2.0** | **Cisco UCS C240 M3S** |  |  |  |
| 2.0.1 | Processor Cisco Server - Intel(R) Xeon(R) CPU E5-2630 v2 @ 2.60GHz; Speed 2600 MHz; 2 CPUs; 6 cores; 12 threads |  |  |  |
| 2.0.2 | Memory Cisco Server - Memory speed 1,6 GHz; Total memory - 98304 MB; Number of memories - 6; Capacity - 16384 MB; DDR3 channel type. |  |  |  |
| 2.0.3 | Power Supply Cisco Server - UCSC-PSU-650W |  |  |  |
| 2.0.4 | NIC - Intel(R) I350 1 Gbps Network Controller |  |  |  |
| 2.0.5 | Controller on System Board - LSI MegaRAID SAS 9271-8i; Cache memory size - 866 MB |  |  |  |
| 2.0.6 | HDD drives capacity - 571250 MB |  |  |  |
| 2.0.7 | SSD drives capacity - 189781 MB |  |  |  |